\\Turn ON the freeze frame:

http://IP\_ADDRESS/rcp.xml?command=0x09A5&type=P\_OCTET&direction=WRITE&num=1&payload=0x8500060135030001

\\Turn OFF the freeze frame:

http://IP\_ADDRESS/rcp.xml?command=0x09A5&type=P\_OCTET&direction=WRITE&num=1&payload=0x8500060135030000