BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
Bosch.Vms.SDK
AlarmCameraActionSetting Class
AlarmCameraActionSetting Properties
AuxCommandNumber Property
Camera Property
IsMoveToPredefinedPositionEnabled Property
IsProtectRecordingEnabled Property
IsSendAuxCommandEnabled Property
IsTriggerRecordingEnabled Property
PredefinedPosition Property

# AlarmCameraActionSetting Properties |

The AlarmCameraActionSetting type exposes the following members.

Properties

| Name | Description
--- | --- | ---
| AuxCommandNumber | The number of the pre-configured auxiliary command (only defined if IsMoveToPredefinedPositionEnabled is true).
| Camera | Camera handle
| IsMoveToPredefinedPositionEnabled | True if the dome camera moves to a predefined position when the alarm is triggered.
| IsProtectRecordingEnabled | True if the alarm recording for the camera gets marked as protected.
| IsSendAuxCommandEnabled | True if the alarm causes the server to send an auxiliary command to the dome camera.
| IsTriggerRecordingEnabled | True if alarm recording is triggered for the camera.
| PredefinedPosition | Returns the number of a predefined dome position (only defined if IsMoveToPredefinedPositionEnabled is true).

Top
See Also

#### Reference

AlarmCameraActionSetting Class
Bosch.Vms.SDK Namespace

Copyright © Bosch Sicherheitssysteme GmbH