BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
Bosch.Vms.SDK
IAlarmConfigurationManager Interface
IAlarmConfigurationManager Methods

# IAlarmConfigurationManager Interface |

This interface gives access to the currently active alarm settings in the BVMS configuration.
Namespace: Bosch.Vms.SDK
Assembly: Bosch.Vms.SDK (in Bosch.Vms.SDK.dll) Version: 1.9.0.0
Syntax
C#
Copy

    public interface IAlarmConfigurationManager

The IAlarmConfigurationManager type exposes the following members.

Methods

| Name | Description
--- | --- | ---
| GetCameraActionSettings | Returns configuration settings for alarm-triggered camera actions related to the type of the given alarm.
| GetImagePaneSettings(AlarmData) | Returns configuration settings for alarm image panes (in the Operator Client) related to the type of the given alarm.
| GetImagePaneSettings(AlarmData, AlarmImagePaneContentType) | Returns configuration settings for alarm image panes related to the type of the given alarm. Only the settings for alarm image panes of the desired content type are returned.

Top
See Also

#### Reference

Bosch.Vms.SDK Namespace

Copyright © Bosch Sicherheitssysteme GmbH