BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
Bosch.Vms.SDK
IDomeCameraManager Interface
IDomeCameraManager Methods
AuxOff Method
AuxOn Method
Focus Method
GetDomeCameraById Method
GetDomeCameraByLogicalNumber Method
GetDomeCameraByName Method
GetDomeCameraInfoList Method
Iris Method
MoveToPredefinedPosition Method
PanTiltZoom Method
SavePosition Method
SendCommand Method
TargetToGeoPosition Method

# IDomeCameraManagerTargetToGeoPosition Method |

Brings given Geo position into camera's view port.
Namespace: Bosch.Vms.SDK
Assembly: Bosch.Vms.SDK (in Bosch.Vms.SDK.dll) Version: 1.9.0.0
Syntax
C#
Copy

    void TargetToGeoPosition(
    	DomeCamera camera,
    	double latitude,
    	double longitude,
    	double height,
    	double zoom
    )

#### Parameters

camera DomeCamera
latitude Double
  Geo latitude (range from -90 to 90).
longitude Double
  Geo longitude (from -180 to 180).
height Double
  Height or altitude of point to be brought into view in meters (from -500 to 1000).
zoom Double
  Zoom factor (range from 1 to 40).

Exceptions

Exception | Condition
--- | ---
SdkException | Thrown if camera doesn't exist in the configuration or is not permitted to caller. Thrown when latitude is not in range from -90 to 90. Thrown when longitude is not in range from -180 to 180. Thrown when height is not in range from -500 to 1000. Thrown when zoom is not in range from 1 to 40.
UnauthorizedAccessSdkException | Thrown if operation is not permitted to caller.

See Also

#### Reference

IDomeCameraManager Interface
Bosch.Vms.SDK Namespace

Copyright © Bosch Sicherheitssysteme GmbH