BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
Bosch.Vms.SDK
ICameraManager Interface
ICameraManager Methods
ExportAsf Method
ExportMov Method
ExportMp4 Method
ExportNative Method
ExportRecordings Method
FindRecordingById Method
FindRecordings Method
GetCameraById Method
GetCameraByLogicalNumber Method
GetCameraByName Method
GetCameraInfoList Method
GetComment Method
GetLogicalNumber Method
GetRecordingMode Method
GetVideoInputNumber Method
IsAttachedToLogicalTree Method
IsBypassed Method
IsGlobalChange Method
IsSignalKnown Method
IsSignalPresent Method
IsSignalTooBlurry Method
IsSignalTooBright Method
IsSignalTooDark Method
IsSignalTooNoisy Method
ProtectRecordings Method
SendData Method
StartAlarmRecording Method
StartManualRecording Method
StartRecording Method
StartRecordingInAlarmMode Method
StartRecordingInManualMode Method
StopAlarmRecording Method
StopManualRecording Method
StopRecording Method
UnprotectRecordings Method

# ICameraManagerSendData Method |

Generates an "External Data Event" for the specified camera.
Namespace: Bosch.Vms.SDK
Assembly: Bosch.Vms.SDK (in Bosch.Vms.SDK.dll) Version: 1.9.0.0
Syntax
C#
Copy

    void SendData(
    	Camera camera,
    	string application,
    	DateTime dateTimeUtc,
    	params string[] data
    )

#### Parameters

camera Camera
  The camera acting as a source of the "External Data Event". Must be a valid, non-null camera from the "Encoders/Decoders" section of Config Clients Events page.
application String
  The application that sends the data. Specify a non-empty string uniquely defining your application. This string will be available from the EventData of the generated event as Key-Value pair by key "Application".
  By using the special application identifier defined by CameraHiddenDataApplicationId, the provided data are hidden in the Operator Client user interface.
dateTimeUtc DateTime
  The current date time in UTC. Defines the Time of the generated event.
data String
  Application specific data. You may specify up to 10 strings. These strings will be available from the EventData of the generated event as Key-Value pairs with keys "Data1", "Data2" up to "Data10". You may not specify null for any of these arguments. Empty strings are allowed.
  When a string begins with the special prefix defined by HiddenAttributePrefix, it defines a "command" to hide one or more peer Key-Value pairs in the Operator Client user interface. The keys must be listed after the prefix, separated with a space. Any Key-Value pair containing a "hide command" is also hidden implicitly.

Exceptions

Exception | Condition
--- | ---
SdkException | Thrown in case camera is null or invalid or not permitted, application is null or empty, data is null, or one of the data-fields have been specified null. Thrown as well if more than 10 data have been provided.

See Also

#### Reference

ICameraManager Interface
Bosch.Vms.SDK Namespace

Copyright © Bosch Sicherheitssysteme GmbH