BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
Bosch.Vms.SDK
TriggeredRecordingData Class
TriggeredRecordingData Properties
Camera Property
PostEventTime Property
PreEventTime Property
RecordingType Property
StartTime Property
StopTime Property

# TriggeredRecordingData Properties |

The TriggeredRecordingData type exposes the following members.

Properties

| Name | Description
--- | --- | ---
| Camera | Camera that has been triggered to start recording.
| PostEventTime | Configured post-event time at the time the recording has been stopped
| PreEventTime | Configured pre-event time at the time the recording has been started
| RecordingType | Type of recording that was triggered.
| StartTime | Requested start time of recording in UTC. Actual recording may have started before this time in the case pre-event recording has been configured for this camera.
| StopTime | UTC time a recording stop has been requested. Actual recording may have continued in the case post-event recording has been configured.

Top
See Also

#### Reference

TriggeredRecordingData Class
Bosch.Vms.SDK Namespace

Copyright © Bosch Sicherheitssysteme GmbH