//From the rcpp documenation - CONF\_PASSWORD\_SETTINGS, 0x028b.

//It exists for CPP6, 7, 7\_3, CPP13, CPP14

//Format for service password

//Name CONF\_PASSWORD\_SETTINGS

//Description Update the service password on devices with a configured service password.

//Method GET

//URL:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

https://DEVICE\_IP/rcp.xml?command=0x028b&type=P\_STRING&direction=WRITE&num=2&payload=DEVICE\_NEW\_PASS

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

//Authentication YES

//Format for live password

//Name CONF\_PASSWORD\_SETTINGS

//Description Update the live password on devices with a configured service password.

//Method GET

//URL;

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

https://DEVICE\_IP/rcp.xml?command=0x028b&type=P\_STRING&direction=WRITE&num=3&payload=DEVICE\_PASS

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

//Authentication YES

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

//For user it is analogical, just num=2