{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Workstations Matrix","Graphic Card Matrix","BVMS OC Perf. single card"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Workstations Matrix","index":0,"n_rows":11,"n_cols":9,"rows_kept":11,"cut":false,"hidden":false,"merged":[[6,0,7,0],[3,3,4,6],[3,8,4,8],[5,1,7,1],[5,2,7,2],[5,3,7,3],[5,4,7,4],[5,5,7,5],[5,7,7,7],[5,6,7,6],[5,8,7,8]]}
[]
[]
[]
[]
[]
[null,"Model","Base Unit","HDD","DVD Drive","Processor","Memory","Service","OS"]
[null,null,"Base Unit"]
[null,null,"Base Unit"]
[null,"Z2G5","HP Z2G5 92%  260W","256 G Z Turbo Drive 2200 TLC","ODD 9.5 DVDWR ","Intel Core i7‑10700 \n(2.9 GHz, 2904 MHz, 8C-CPU)","8GB DDR4-3200 UDIMM NECC (1x8GB) RAM","HP 3‑year Next Business Day on-site hardware support","Microsoft Windows 10 Pro Edition 20H2, 64-Bit"]
[null,"Z4G4","HP Z4G4  750W 90 %","500GB 7200 RPM SATA","SuperMulti DVD RW SATA","Intel Xeon W-2123 \n(3,6 GHz, 2.666 MHz,\n8,25 MB, 4C-CPU)","8GB DDR4-2666 ECC (1x8GB) RAM","HP 3‑year Next Business Day on-site hardware support","Microsoft Windows 10 Pro Edition 20H2, 64-Bit"]
[null,"DIP 7000 AIO 3rd Gen (DIP-73XS)",null,"Intel Raid 1 223.44 GB (SSD)\nAVAGO SMC3108 SCSI Raid","TEAC DV-W28S-F DVD Drive","Intel Xeon E-2226 GE (3.40 GHz, 3408 Mhz, 6C CPU)","16GB DDR4-2666 NECC (1x16GB) RAM",null,"Microsoft Windows Server 2019 Standard"]

{"sheet":"Graphic Card Matrix","index":1,"n_rows":15,"n_cols":9,"rows_kept":15,"cut":false,"hidden":false,"merged":[[14,2,15,3],[5,7,7,7],[6,0,7,0],[8,1,9,1],[10,1,11,1],[3,1,4,8],[5,1,7,1],[5,3,7,3],[5,4,7,4],[5,5,7,5],[5,6,7,6],[5,8,7,8],[5,2,7,2]]}
[]
[]
[]
[]
[]
[null,"Workstation  ","Graphic cards","Application","Description","No of cards supported","Maximum monitors  per card","Max monitors per WS (1)","GPU Decoding Supported"]
[null,"CTN","CTN"]
[null,"CTN","CTN"]
[null,"Z2G5",null,"Entry 3D Graphics Card","Intel UHD Graphics 630","No 2nd card supported",2,2,"yes"]
[null,null,null,"Mid-Range 3D Graphics Card","NVIDIA Quadro P620 (2 GB)","No 2nd card supported",4,4,"yes"]
[null,"Z4G4",null,"High-End 3D Graphics Card","NVIDIA Quadro P2200 (5GB)","No 2nd card supported",4,4,"yes"]
[null,null,null,"High-End 3D Graphics Card","NVIDIA Quadro RTX 4000 (8GB)","No 2nd card supported",4,4,"yes"]
[null,"DIP 7000 AIO 3rd Gen",null,"Mid-Range 3D Graphics Card","Intel UHD Graphics P630","No 2nd card supported",2,2,"no"]
[]
[null,null,"(1) BVMS uses a maximum of 4 monitors\n(2) multiple cards of the same typ"]

{"sheet":"BVMS OC Perf. single card","index":2,"n_rows":19,"n_cols":24,"rows_kept":19,"cut":false,"hidden":false,"merged":[[3,1,4,22],[7,6,7,7],[7,8,7,9],[6,6,6,9],[6,10,6,13],[7,10,7,11],[7,12,7,13],[7,18,7,19],[6,18,6,19],[6,20,6,21],[7,20,7,21],[6,22,6,23],[7,22,7,23],[6,14,6,15],[7,14,7,15],[5,18,5,23],[6,1,7,1],[18,2,18,22],[7,16,7,17],[6,16,6,17],[8,1,9,1],[10,1,11,1],[5,4,5,17],[6,4,7,5],[6,24,7,24],[6,3,7,3],[6,2,7,2]]}
[]
[]
[]
[]
[]
[null,null,null,null,"H.264, Default Profile \"Balanced standard\" ",null,null,null,null,null,null,null,null,null,null,null,null,null,"H.265 Default Profile \"Balanced standard\" "]
[null,"Workstation  ","Graphic cards","Description","25fps 480p (VGA /2CIF) ",null,"720p",null,null,null,"1080p",null,null,null,"5MP",null,"4K",null,"720p",null,"1080p",null,"5MP"]
[null,"CTN","CTN",null,null,null,"30 fps ",null,"60 fps ",null,"30 fps ",null,"60 fps ",null,"12 fps",null,"3840x2160",null,"30 fps",null,"30 fps",null,"30 fps"]
[null,"Z2G5","NG","Intel UHD Graphics 630","50",null,"22"," +G",10," +G",10," +G",6," +G",9," +G",3," +G",26," +G","12"," +G","5"," +G"]
[null,null,"Nvidia","NVIDIA Quadro P620 (2 GB)",60,null,32," +G",16," +G",20," +G",10," +G",16," +G",5," +G",32," +G",16," +G",8," +G"]
[null,"Z4G4","Nvidia","NVIDIA Quadro P2200 (5GB)",70,null,34," +G",16," +G",22," +G",12," +G",20," +G","6"," +G",34," +G","19"," +G","8"," +G"]
[null,null,"Nvidia","NVIDIA Quadro RTX 4000 (8GB)",70,null,30," +G",14," +G",24," +G",13," +G",18," +G",6," +G",32," +G",20," +G",10," +G"]
[null,"DIP 7000 AIO 3rd Gen","NG","Intel UHD Graphics P 630",40,null,"15",null,"6",null,"7",null,"4",null,"8",null,"2",null,"12",null,"5",null,"2"]
[null,"Max CPU Load:","> 90%","Max CPU Load DIP:","> 90%"]
[null,"oder Framedrops:","> 5%","oder Framedrops:","> 5%"]
[]
[null,"Attention:","since BVMS 9.0 the values have been measured with different settings than in previous versions."]
[]
[null,"Note 1)","Limit is determined by reaching either more than 90 % CPU or more than 5% framedrops, each exceeded in more than 5 out of 10 measurements. \nImage decoder must not be in an overload situation, cameos must appear fluent."]