BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
Bosch.Vms.SDK
AlarmData Class
AlarmData Properties
AlarmId Property
ColorArgb Property
Comment Property
CreationTimeUtc Property
Device Property
DisplayName Property
Priority Property
ServerId Property
State Property

# AlarmData Properties |

The AlarmData type exposes the following members.

Properties

| Name | Description
--- | --- | ---
| AlarmId | BVMS internal Id of the alarm.
| ColorArgb | Alarm color. Specifies in which color the alarm entry shall be displayed in the BVMS Operator Client's alarm list.
| Comment | Comment.
| CreationTimeUtc | The date and time when the alarm was created.
| Device | SDK Device which originated the alarm. It can be null in case of an internal error.
| DisplayName | Title of the alarm.
| Priority | Alarm priority. The alarm priority specifies whether this alarm will show up in the BVMS Operator Client as a "popup alarm". A popup alarm will automatically display configured Image pane contents. The smaller the value of this property, the higher the alarm priority.
| ServerId | Server Id.
| State | Alarm state.

Top
See Also

#### Reference

AlarmData Class
Bosch.Vms.SDK Namespace

Copyright © Bosch Sicherheitssysteme GmbH