BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
Bosch.Vms.SDK
IMatrixManager Interface
IMatrixManager Methods
DisplayCamera Method
GetCameras Method
GetMatrixById Method
GetMatrixByName Method
GetMatrixInfoList Method
IsCameraDisplayable Method
SendCommand Method
SequenceBackward Method
SequenceForward Method
SequenceHold Method
SequenceLoad Method
SequenceRun Method
SequenceUnload Method
SetOsdMessage Method

# IMatrixManagerSendCommand Method |

Sends an Allegiant CCL command to the Allegiant matrix
Namespace: Bosch.Vms.SDK
Assembly: Bosch.Vms.SDK (in Bosch.Vms.SDK.dll) Version: 1.9.0.0
Syntax
C#
Copy

    void SendCommand(
    	Matrix m,
    	string command
    )

#### Parameters

m Matrix
command String

Exceptions

Exception | Condition
--- | ---
UnauthorizedAccessSdkException | Thrown if operation is not permitted to caller.

Remarks
To use the CCL commands you need the CCL User Guide. This manual is available in the Online Product Catalog in the document section of each LTC Allegiant Matrix.
See Also

#### Reference

IMatrixManager Interface
Bosch.Vms.SDK Namespace

Copyright © Bosch Sicherheitssysteme GmbH