BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
BVMS Server- and Client-SDK
Bosch.Vms.SDK
IMatrixManager Interface
IMatrixManager Methods
DisplayCamera Method
GetCameras Method
GetMatrixById Method
GetMatrixByName Method
GetMatrixInfoList Method
IsCameraDisplayable Method
SendCommand Method
SequenceBackward Method
SequenceForward Method
SequenceHold Method
SequenceLoad Method
SequenceRun Method
SequenceUnload Method
SetOsdMessage Method

# IMatrixManager Methods |

The IMatrixManager type exposes the following members.

Methods

| Name | Description
--- | --- | ---
| DisplayCamera | Displays the given Camera on a monitor connected to a Matrix
| GetCameras | returns all cameras that are connected to the matrix m
| GetConnectionState | Gets the ConnectionState of a device. (Inherited from IDeviceManager)
| GetDeviceById | Retrieves device handle by ID. (Inherited from IDeviceManager)
| GetDeviceByName | Retrieves device handle by name. (Inherited from IDeviceManager)
| GetDeviceInfoList | Gets information about all devices. (Inherited from IDeviceManager)
| GetInitialStates | Triggers submission of current device state events to registered event receivers. (Inherited from IDeviceManager)
| GetMatrixById | Gets the Allegiant matrix device corresponding to the given GUID
| GetMatrixByName | Gets the Allegiant matrix device corresponding to the given display name
| GetMatrixInfoList | Gets information for all matrix devices
| GetName | Retrieves device name. (Inherited from IDeviceManager)
| IsCameraDisplayable | returns true if Camera c is connected to the Matrix m and can therefore be displayed
| SendCommand | Sends an Allegiant CCL command to the Allegiant matrix
| SequenceBackward | Sets the currently loaded sequence one step back
| SequenceForward | Forwards the currently loaded sequence one step
| SequenceHold | Holds the currently loaded sequence on that monitor
| SequenceLoad | Loads a sequence for a monitor
| SequenceRun | Starts the currently loaded sequence on that monitor
| SequenceUnload | Unloads the currently loaded sequence for that monitor
| SetOsdMessage | Sets the OSD message for the specified monitor

Top
See Also

#### Reference

IMatrixManager Interface
Bosch.Vms.SDK Namespace

Copyright © Bosch Sicherheitssysteme GmbH