{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Workstations Matrix","Graphic Card Matrix","BVMS OC Perf. single card"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Workstations Matrix","index":0,"n_rows":14,"n_cols":9,"rows_kept":14,"cut":false,"hidden":false,"merged":[[6,0,7,0],[3,3,4,6],[3,8,4,8],[5,1,7,1],[5,2,7,2],[5,3,7,3],[5,4,7,4],[5,5,7,5],[5,7,7,7],[5,6,7,6],[5,8,7,8]]}
[]
[]
[]
[]
[]
[null,"Model","Base Unit","HDD","DVD Drive","Processor","Memory","Service","OS"]
[null,null,"Base Unit"]
[null,null,"Base Unit"]
[null,"Z2G9","HP Z2G9 SFF 450W","256GB PCIe-4x4 2280 M.2 SSD","ODD 9.5 DVDWR ","Intel Core i7-12700 \n(2.10G 25MB 12 cores)","16GB (2x8GB) DDR5 4800 RAM","HP 5‑year Next Business Day on-site hardware support","Microsoft Windows 10 Pro Edition 20H2, 64-Bit"]
[null,"Z2G5","HP Z2G5 92%  260W","256GB Z Turbo Drive 2200 TLC","ODD 9.5 DVDWR ","Intel Core i7‑10700 \n(2.9 GHz, 2904 MHz, 8C-CPU)","8GB DDR4-3200 UDIMM NECC (1x8GB) RAM","HP 3‑year Next Business Day on-site hardware support","Microsoft Windows 10 Pro Edition 20H2, 64-Bit"]
[null,"Z4G4","HP Z4G4  750W 90 %","500GB 7200 RPM SATA","SuperMulti DVD RW SATA","Intel Xeon W-2223 \n(3,6 GHz, 2.666 MHz,\n8,25 MB, 4C-CPU)","16 GB DDR4-2666 ECC (2x8GB) RAM","HP 3‑year Next Business Day on-site hardware support","Microsoft Windows 10 Pro Edition 20H2, 64-Bit"]
[null,"DIP 5000 AIO\n(DIP-52xx)","DIP-524W","238.35 GB KXG50ZNV256G TOSHIBA",null,"Intel(R) Core(TM) i3-8100 CPU @ 3.60GHz, 3600 MHz, 4 Core(s), 4 Logical Processor(s)","8GB",null,"Windows Storage Server 2016 Workgroup\n1607 "]
[null,"DIP 7000 AIO\n(DIP-72xx)","DIP-728S","212.27 GB Intel Raid 1 Volume","TEAC DV-W28S-F","Intel(R) Xeon(R) CPU E3-1275 v3 @ 3.50GHz, 3500 Mhz, 4 Core(s), 8 Logical Processor(s)","8GB DDR3",null,"Windows Storage Server 2016 Standard\n1607"]
[null,"DIP 7000 AIO 3rd Gen (DIP-73XS)","DIP-73XS","Intel Raid 1 223.44 GB (SSD)\nAVAGO SMC3108 SCSI Raid","TEAC DV-W28S-F DVD Drive","Intel Xeon E-2226 GE (3.40 GHz, 3408 Mhz, 6C CPU)","16GB DDR4-2666 NECC (1x16GB) RAM",null,"Microsoft Windows Server 2019 Standard\n1809"]

{"sheet":"Graphic Card Matrix","index":1,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[[6,0,7,0],[16,1,17,1],[3,1,4,8],[5,1,7,1],[5,3,7,3],[5,4,7,4],[5,5,7,5],[5,6,7,6],[5,8,7,8],[5,2,7,2],[5,7,7,7],[12,1,15,1],[9,1,11,1]]}
[]
[]
[]
[]
[]
[null,"Workstation  ","Graphic cards","Application","Description","No of cards supported","Maximum monitors  per card","Max monitors per WS (1)","GPU Decoding Supported"]
[null,"CTN","CTN"]
[null,"CTN","CTN"]
[null,"Z2G9","NVIDIA",null,"NVIDIA T400 (4GB)","No 2nd card supported",3,3,"yes"]
[null,"Z2G5","NG","Entry 3D Graphics Card","INTEL UHD Graphics 630","No 2nd card supported",2,2,"yes"]
[null,null,"NVIDIA","Mid-Range 3D Graphics Card","NVIDIA Quadro P620 (2 GB)","No 2nd card supported",4,4,"yes"]
[null,null,"NVIDIA",null,"NVIDIA T600 (4GB)","No 2nd card supported",4,4,"yes"]
[null,"Z4G4","NVIDIA",null,"NVIDIA T600 (4GB)",null,4,4,"yes"]
[null,null,"NVIDIA","High-End 3D Graphics Card","NVIDIA T1000 (4GB)",null,4,4,"yes"]
[null,null,"NVIDIA",null,"NVIDIA RTX A 2000 (12 GB)",null,4,4,"yes"]
[null,null,"NVIDIA","High-End 3D Graphics Card","NVIDIA RTX A 4000 (16 GB)",null,4,4,"yes"]
[null,"DIP 5000 AIO\n(DIP-52xx)","NG",null,"INTEL UHD Graphics 630","No 2nd card supported",3,3,"no"]
[null,null,"NVIDIA",null,"NVIDIA Quadro P620 (2 GB)","No 2nd card supported",4,4,"yes"]
[null,"DIP 7000 AIO\n(DIP-72xx)","NVIDIA",null,"NVIDIA Quadro P620 (2 GB)","No 2nd card supported",4,4,"yes"]
[null,"DIP 7000 AIO\n3rd Gen","NG","Mid-Range 3D Graphics Card","INTEL UHD Graphics P630","No 2nd card supported",3,3,"no"]
[]
[]
[]
[]
[null,null,"(1) BVMS uses a maximum of 4 monitors"]

{"sheet":"BVMS OC Perf. single card","index":2,"n_rows":26,"n_cols":24,"rows_kept":26,"cut":false,"hidden":false,"merged":[[25,2,25,22],[5,4,5,17],[6,4,7,5],[6,24,7,24],[6,3,7,3],[6,2,7,2],[6,1,7,1],[24,2,24,22],[7,16,7,17],[6,16,6,17],[15,1,16,1],[11,1,14,1],[22,2,22,22],[9,1,10,1],[3,1,4,22],[7,6,7,7],[7,8,7,9],[6,6,6,9],[6,10,6,13],[7,10,7,11],[7,12,7,13],[7,18,7,19],[6,18,6,19],[6,20,6,21],[7,20,7,21],[6,22,6,23],[7,22,7,23],[6,14,6,15],[7,14,7,15],[5,18,5,23]]}
[]
[]
[]
[]
[]
[null,null,null,null,"H.264, Default Profile \"Balanced standard\" ",null,null,null,null,null,null,null,null,null,null,null,null,null,"H.265 Default Profile \"Balanced standard\" "]
[null,"Workstation  ","Graphic cards","Description","25fps 480p (VGA /2CIF) ",null,"720p",null,null,null,"1080p",null,null,null,"5MP",null,"4K",null,"720p",null,"1080p",null,"5MP"]
[null,"CTN","CTN",null,null,null,"30 fps ",null,"60 fps ",null,"30 fps ",null,"60 fps ",null,"12 fps",null,"3840x2160",null,"30 fps",null,"30 fps",null,"30 fps"]
[null,"Z2G9","Nvidia","T400 (4GB)","81",null,"32","+G",17,"+G",23,"+G",13,"+G",18,"+G",6,"+G",33,"+G","29","+G","11","+G"]
[null,"Z2G5","Nvidia","NVIDIA Quadro P620 (2 GB)",60,null,32,"+G",16,"+G",20,"+G",10,"+G",12,"+G",5,"+G",32,"+G",16,"+G",8,"+G"]
[null,null,"Nvidia","Nvidia T600 (4GB)","59",null,"31","+G",15,"+G",20,"+G",10,"+G",17,"+G",5,"+G",30,"+G","19","+G","11","+G"]
[null,"Z4G4","Nvidia","Nvidia T600 (4GB)",59,null,31,"+G",15,"+G",28,"+G",11,"+G",12,"+G",7,"+G",25,"+G",20,"+G",12,"+G"]
[null,null,"Nvidia","NVIDIA Quadro T1000 (4 GB)",60,null,32,"+G",16,"+G",30,"+G",12,"+G",15,"+G",8,"+G",29,"+G","23","+G","14","+G"]
[null,null,"Nvidia","NVIDIA RTX A 2000 (12 GB)",65,null,27,"+G",14,"+G",24,"+G",11,"+G",22,"+G",7,"+G",30,"+G",22,"+G",12,"+G"]
[null,null,"Nvidia","NVIDIA RTX A 4000 (16 GB)",55,null,27,"+G",14,"+G",24,"+G",11,"+G",22,"+G",8,"+G",31,"+G","22","+G","15","+G"]
[null,"DIP 5000 AIO\n(DIP-52xx)","NG","Intel UHD Graphics 630",28,null,11,null,5,null,5,null,2,null,6,null,1,null,8,null,4,null,2]
[null,null,"Nvidia","NVIDIA Quadro P620 (2 GB)",30,null,19,"+G",9,"+G",13,"+G",7,"+G",12,"+G",4,"+G",19,"+G","12","+G","6","+G"]
[null,"DIP 7000 AIO\n(DIP-72xx)","Nvidia","NVIDIA Quadro P620 (2 GB)",35,null,23,"+G",13,"+G",15,"+G",7,"+G",11,"+G",4,"+G",22,"+G",14,"+G",6,"+G"]
[null,"DIP 7000 AIO 3rd Gen","NG","Intel UHD Graphics P 630",40,null,15,null,7,null,8,null,3,null,8,null,2,null,11,null,"5",null,"2"]
[null,"Max CPU Load:","> 90%","Max CPU Load DIP:","> 90%"]
[null,"oder Framedrops:","> 5%","oder Framedrops:","> 5%"]
[]
[null,"Attention:","When using the new GPUs T1000, RTX A2000 and RTX A4000 in configurations with BVMS, we recommend enabling the Hardware-accelerated GPU scheduling feature in Windows. This will enable the system to avoid the time-out detection recovery feature (TDR) which can be activated when opening higher numbers of cameos."]
[]
[null,"Note 1)","Limit is determined by reaching either more than 90 % CPU or more than 5% framedrops, each exceeded in more than 5 out of 10 measurements. \nImage decoder must not be in an overload situation, cameos must appear fluent."]
[null,"Note 2)","+G callout means that in addition to CPU decoding (software) also the GPU decoding (hardware) is active."]