{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["BVMS OC Perf. single card","Workstations Matrix","Graphic Card Matrix"],"not_rendered":{"images":1,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"BVMS OC Perf. single card","index":0,"n_rows":25,"n_cols":15,"rows_kept":25,"merged":[[3,1,4,13],[5,5,5,8],[5,9,5,14],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,7,4],[6,5,7,6],[6,7,6,8],[6,9,6,10],[6,11,6,12],[6,13,6,14],[6,15,7,15],[7,7,7,8],[7,9,7,10],[7,11,7,12],[7,13,7,14],[20,2,20,13],[22,2,22,13],[23,2,23,13]]}
[]
[]
[]
[]
[]
[{"$nulls":5},"H.264, Default Profile \"Balanced standard\" ",{"$nulls":3},"H.265 Default Profile \"Balanced standard\" "]
[null,"Workstation  ","Verified with BVMS version  ","Graphic cards","Description","480p (VGA /2CIF) \n30 fps",null,"4K",null,"720p",null,"1080p",null,"4K"]
[null,"CTN","CTN","CTN",{"$nulls":3},"30 fps",null,"30 fps",null,"30 fps",null,"30 fps"]
[null,"Z2G1i  \nMHW-WZ2G1I-GPU","14.0.0\n13.1.0\n13.0.0","Nvidia","A400 (4GB)","64",null,"8","+G","30","+G","25","+G","7","+G"]
[null,"Z2G9  \nMHW-WZ2G9-GPU","14.0.0\n13.1.0\n13.0.0","Nvidia","T400 (4GB)","64",null,"7","+G","30","+G","25","+G","7","+G"]
[null,"Z4G5\nMHW-WZ4G5-HEN3","14.0.0\n13.1.0\n13.0.0","Nvidia","NVIDIA A1000 (8 GB)","64",null,"12","+G","38","+G","27","+G","12","+G"]
[null,"Z4G5\nMHW-WZ4G5-HEN3","14.0.0\n13.1.0\n13.0.0","Nvidia","NVIDIA Quadro T1000 (8 GB)","64",null,"8","+G","33","+G","27","+G","8","+G"]
[null,"Z4G4 (EOL)\nMHW-WZ4G4-HEN2\nMHW-WZ4G4-HEN4","14.0.0\n13.1.0\n13.0.0","Nvidia","NVIDIA Quadro T1000 (4 GB)","60",null,"7","+G","35","+G","30","+G","8","+G"]
[null,"DIP aio 4000\n(DIP-44xx)","14.0.0\n13.1.0\n13.0.0","NG","Intel UHD Graphics 630","20",null,1,null,10,null,"4",null,"1"]
[null,"DIP aio 6000\n(DIP-64xx)","14.0.0\n13.1.0\n13.0.0","NG","Intel UHD Graphics 630","20",null,1,null,10,null,"4",null,"1"]
[null,"DIP aio 7000 3rd Gen\n(DIP-73xx)","14.0.0\n13.1.0\n13.0.0","NG","Intel UHD Graphics P 630","21",null,2,null,13,null,"6",null,"1"]
[null,"DIP aio 7000 4th Gen\n(DIP-74xx)","14.0.0\n13.1.0\n13.0.0","NG","Intel UHD Graphics P 770","35",null,2,null,20,null,"14",null,"1"]
[null,"Max CPU Load:",null,"> 90%","Max CPU Load DIP:","> 90%"]
[null,"oder Framedrops:",null,"> 5%","oder Framedrops:","> 5%"]
[]
[null,"Attention:","When using the new GPUs T1000, RTX A2000 and RTX A4000 in configurations with BVMS, we recommend enabling the Hardware-accelerated GPU scheduling feature in Windows 10 (in Windows 11 it is by default already enabled). This will enable the system to avoid the time-out detection recovery feature (TDR) which can be activated when opening higher numbers of cameos."]
[]
[null,"Note 1)","Limit is determined by reaching either more than 90 % CPU or more than 5% framedrops, each exceeded in more than 5 out of 10 measurements. \nImage decoder must not be in an overload situation, cameos must appear fluent."]
[null,"Note 2)","+G callout means that in addition to CPU decoding (software) also the GPU decoding (hardware) is active."]
[null,"Note 3)","This table should only be used as a reference. Actual decoding performance might depend on specifics of the system and multiple variables, like detailed recording profile settings, movement in the scene, etc."]

{"sheet":"Workstations Matrix","index":1,"n_rows":18,"n_cols":9,"rows_kept":18,"merged":[[3,3,4,6],[3,8,4,8],[5,1,7,1],[5,2,7,2],[5,3,7,3],[5,4,7,4],[5,5,7,5],[5,6,7,6],[5,7,7,7],[5,8,7,8],[6,0,7,0]]}
[]
[]
[]
[]
[]
[null,"Model","Base Unit","HDD","DVD Drive","Processor","Memory","Service","OS"]
[null,null,"Base Unit"]
[null,null,"Base Unit"]
[null,"Z2G1i","HP Z2G1i SFF 450W","256GB PCIe-4x4 2280 M.2 SSD","ODD 9.5 DVDWR ","Intel Core i7-12700 \n(2.10G 25MB 12 cores)","16GB (2x8GB) DDR5 4800 RAM","HP 5‑year Next Business Day on-site hardware support","Microsoft Windows 11 Pro, \n64-Bit"]
[null,"Z2G9","HP Z2G9 SFF 450W","256GB PCIe-4x4 2280 M.2 SSD","ODD 9.5 DVDWR ","Intel Core i7-12700 \n(2.10G 25MB 12 cores)","16GB (2x8GB) DDR5 4800 RAM","HP 5‑year Next Business Day on-site hardware support","Microsoft Windows 11 Pro, 64-Bit"]
[null,"Z2G5 (EOL)","HP Z2G5 92%  260W","256GB Z Turbo Drive 2200 TLC","ODD 9.5 DVDWR ","Intel Core i7‑10700 \n(2.9 GHz, 2904 MHz, 8C-CPU)","8GB DDR4-3200 UDIMM NECC (1x8GB) RAM","HP 3‑year Next Business Day on-site hardware support","Microsoft Windows 10 Pro Edition 20H2, 64-Bit"]
[null,"Z4G5","HP Z4G5 525W ","512GB PCIe-4x4   2280 TLC M.2 SSD","ODD 9.5 DVDWR ","Intel Xeon W3-2423 (2.10G 15MB 6 cores 120W CPU)","16GB (1x16GB) DDR5 4800 DIMM ECC REG Memory","HP 5‑year Next Business Day on-site hardware support","Microsoft Windows 11 Pro 64 for Workstations 6 Cores"]
[null,"Z4G4 (EOL)","HP Z4G4  750W 90 %","500GB 7200 RPM SATA","SuperMulti DVD RW SATA","Intel Xeon W-2223 \n(3,6 GHz, 2.666 MHz,\n8,25 MB, 4C-CPU)","16 GB DDR4-2666 ECC (2x8GB) RAM","HP 3‑year Next Business Day on-site hardware support","Microsoft Windows 10 Pro Edition 20H2, 64-Bit"]
[null,"DIP 4000 AIO\n(DIP-44xx)","DIP-44xx","256 GB M.2 SSD\n2x SATA3 3.5 inch 7200 rpm HDD",null,"Intel® Core™ i3-10100E\n@ 3.20 GHz","8GB DDR4-2666 1RX8 LP SODIMM",null,"Microsoft Windows Server IoT 2022\nfor Storage Workgroup"]
[null,"DIP 6000 AIO (DIP-64xx)","DIP-64xx","256 GB M.2 SSD\nSAS RAID Card 12Gb/s Eight-Port\n4x SATA3 3.5 inch 7200 rpm HDD",null,"Intel® Core™ i3-10100E\n@ 3.20 GHz","16GB DDR4-2933 2Rx8 ECC\nUDIMM\nECC unbuffered",null,"Microsoft Windows Server IoT 2022\nfor Storage Workgroup"]
[null,"DIP 5000 AIO\n(DIP-52xx)","DIP-524W","238.35 GB KXG50ZNV256G TOSHIBA",null,"Intel(R) Core(TM) i3-8100 CPU @ 3.60GHz, 3600 MHz, 4 Core(s), 4 Logical Processor(s)","8GB",null,"Windows Storage Server 2016 Workgroup\n1607 "]
[null,"DIP 7000 AIO\n(DIP-72xx)","DIP-728S","212.27 GB Intel Raid 1 Volume","TEAC DV-W28S-F","Intel(R) Xeon(R) CPU E3-1275 v3 @ 3.50GHz, 3500 Mhz, 4 Core(s), 8 Logical Processor(s)","8GB DDR3",null,"Windows Storage Server 2016 Standard\n1607"]
[null,"DIP 7000 AIO 3rd Gen (DIP-73XS)","DIP-73XS","Intel Raid 1 223.44 GB (SSD)\nAVAGO SMC3108 SCSI Raid","TEAC DV-W28S-F DVD Drive","Intel Xeon E-2226 GE (3.40 GHz, 3408 Mhz, 6C CPU)","16GB DDR4-2666 NECC (1x16GB) RAM",null,"Microsoft Windows Server 2019 Standard\n1809"]

{"sheet":"Graphic Card Matrix","index":2,"n_rows":26,"n_cols":9,"rows_kept":26,"merged":[[3,1,4,8],[5,1,7,1],[5,2,7,2],[5,3,7,3],[5,4,7,4],[5,5,7,5],[5,6,7,6],[5,7,7,7],[5,8,7,8],[6,0,7,0],[9,1,11,1],[13,1,16,1],[17,1,18,1]]}
[]
[]
[]
[]
[]
[null,"Workstation  ","Graphic cards","Application","Description","No of cards supported","Maximum monitors  per card","Max monitors per WS (1)","GPU Decoding Supported"]
[null,"CTN","CTN"]
[null,"CTN","CTN"]
[null,"Z2G9","NVIDIA",null,"NVIDIA T400 (4GB)","No 2nd card supported",3,3,"yes"]
[null,"Z2G5 (EOL)","NG","Entry 3D Graphics Card","INTEL UHD Graphics 630","No 2nd card supported",2,2,"yes"]
[null,null,"NVIDIA","Mid-Range 3D Graphics Card","NVIDIA Quadro P620 (2 GB)","No 2nd card supported",4,4,"yes"]
[null,null,"NVIDIA",null,"NVIDIA T600 (4GB)","No 2nd card supported",4,4,"yes"]
[null,"Z4G5","NVIDIA",null,"NVIDIA T1000 (8GB)",null,4,4,"yes"]
[null,"Z4G4 (EOL)","NVIDIA",null,"NVIDIA T600 (4GB)",null,4,4,"yes"]
[null,null,"NVIDIA","High-End 3D Graphics Card","NVIDIA T1000 (4GB)",null,4,4,"yes"]
[null,null,"NVIDIA",null,"NVIDIA RTX A 2000 (12 GB)",null,4,4,"yes"]
[null,null,"NVIDIA","High-End 3D Graphics Card","NVIDIA RTX A 4000 (16 GB)",null,4,4,"yes"]
[null,"DIP 5000 AIO\n(DIP-52xx)","NG",null,"INTEL UHD Graphics 630","No 2nd card supported",3,3,"no"]
[null,null,"NVIDIA",null,"NVIDIA Quadro P620 (2 GB)","No 2nd card supported",4,4,"yes"]
[null,"DIP 7000 AIO\n(DIP-72xx)","NVIDIA",null,"NVIDIA Quadro P620 (2 GB)","No 2nd card supported",4,4,"yes"]
[null,"DIP 7000 AIO\n3rd Gen","NG","Mid-Range 3D Graphics Card","INTEL UHD Graphics P630","No 2nd card supported",3,3,"no"]
[null,"DIP 4000 AIO \n(DIP-44xx)","NG",null,"Intel UHD Graphics 630","No 2nd card supported",3,3,"no"]
[null,"DIP 6000 AIO \n(DIP-64xx)","NG","Mid-Range 3D Graphics Card","Intel UHD Graphics 630","No 2nd card supported",3,3,"no"]
[]
[]
[null,null,"(1) BVMS uses a maximum of 4 monitors"]